| **SL** | **Safety Gear** | **Specification** |
| --- | --- | --- |
| 01. | **Hand Sanitizer** | Size: 100ml  Composition: 70% Alcohol (Ethanol + IPE),  Carbomer, Glycerin, Polyethylene Glycol. TEA, Aqua & Perfume. |
| 02. | **Face Mask** | Three-layer antibacterial fabric, both side elastic ear loop, Best quality ceiling & swing, Washable & Reusable, Packets separately.  Preferable types of fabrics, number of layers and the composition of a non-medical, fabric mask:   * Two layers of absorbent material such as cotton * Additional spider layer over the outer layer for extra protection |
| 03 | **Safety Goggles** | Made with Nylon frame and Polycarbonate lens which offers lighter, exceptional impact and splash protection with excellent vision, combined with ultimate eye safety. It must have anti-fog feature. |
| 04. | **Hand Gloves** | Chemical resistant, nitrile gloves (industrial) having flock lined inners, diamond finish grip, straight cuff. Should be reusable and washable. |
| 05. | **Reflective Safety Vest** | 120 gsm fabric, Both side high visible reflecting tape, high quality zipper, unisex & free size, high quality ceiling & swing. Washable & Reusable. Packets separately. |
| 06. | **Full-Body Apron** | 210 gsm fabric, high quality zipper & Velcro, unisex, high quality ceiling & swing. Washable & reusable. Packets separately. It should have:   * One full pant and one full sleeve shirt with hoody * Adhesive flap over the zipper of the upper body part * Sigle way zipper * Elasticated hood, wrists, ankles & waist. |
| 07. | **Safety Gumboot** | Material: PVC  Requirements: full length and soft texture, with steel toe, puncture resistance, oil/acid/chemical resistant and waterproof, no leakage when air with pressure of 0.15 Kg is forced into the boots, antiskid, antistatic, closed hill, cleated outsole, inside fabric lining for maximum comfort.  Different sizes of safety gumboots are required to be provided. Additional 500 pairs of safety gumboots of different sizes would be required to be sent to the target cities – unused pairs will be returned to the vendor. |
| 08. | **Safety Shoe** | Protective footwear having steel toe with upper body made out of grain leather/artificial leather and polyurethane outsole for protection against physical hazards.  Other requirements: ankle length shoes, antiskid, antistatic, closed hill, water repellent uppers, puncture resistance, cleated outsole.  Different sizes of safety shoes are required to be provided. Additional 1000 pairs of safety shoes of different sizes would be required to be sent to the target cities – unused pairs will be returned to the vendor.  *Note: Not needed by the emptiers. BTW, original leather shoes last longer.* |
| 09 | **Safety Helmet** | Requirements:   * With shell made out of ABS; with high quality headband, harness, sweatband, peak and chinstrap * ventilated slots, easy adjustable chin strap, easy replacement of chin strap, comfortable reset system to fit with head |

**This specification sheet is provided to the trainers for familiarizing themselves with the technical terms and aspect required to consider before ordering PPE for sanitation workers. In top, users ( Sanitation workers ) comfort , prior consultation with sample may fix the gap in future.**